New supported models: { [DC155], [DC161*β], [DC162*β], [DC163] }. 

Note (*β): This model has not been fully tested and is only provided as a beta, to be used at 
the user's own risk. In case of problems, support can only be provided by stethos, not by Ricoh. 

New features: 
 - convert (in new v13.1): (in GWNX, GWL, sGW, ARM-QB.sGW): none 
 - IBS-CC (in v8.3.3.0): 
 - PJL file permission in WIM temporarily toggled to “Permit” during installation 
 - new Quicksets: 
 - "Prevention against unauthorized copying (PJL) 
 - "Prevention against unauthorized copying (no PJL) 

Bug fixes: 
 - convert (in new v13.1): (in GWNX, GWL, sGW, ARM-QB.sGW): none 
 - IBS-CC (in v8.3.3.0):n 
 - "SNMP Retries" setting was ignored 
 - hang of Single-click Installation if WIM access fails 
 - ibs.main/.gps/.bootup: 
 - slow debug file read-back via IBS-CC 