PCL Printer Driver
For Microsoft Windows Server 2008, Windows 7, Windows Server 2008 R2, Windows Server 2012, Windows 8.1, Windows Server 2012 R2, Windows 10, Windows Server 2016, Windows Server 2019
(x86/x64)

SOFTWARE LICENSE AGREEMENT
YOU, THE END USER, SHALL USE THIS SOFTWARE("THE SOFTWARE") ACCORDING TO THE TERMS OF THIS AGREEMENT.
BY LOADING THE SOFTWARE INTO ANY COMPUTER, YOU ARE AGREEING TO BE BOUND BY THESE TERMS. IF YOU DO NOT ACCEPT THE TERMS OF THIS AGREEMENT, YOU MAY NOT LOAD THIS SOFTWARE INTO ANY COMPUTER.
Grant of License
The Software is licensed for use by you for the equipment packaged with the Software or designated by its supplier ("the equipment"). You are permitted to use the Software on any computer which permits electronic access to the equipment. You are not permitted to rent or lease the Software or to transfer your rights under this license to a third party.
Acceptance
You shall be deemed to have accepted the terms of this Agreement by loading the Software into any computer.
Duration
This license is effective until terminated. The license will terminate where you fail to comply with the terms of this Agreement. Upon termination, you agree to destroy all copies of the Software and its documentation.
Ownership of Software
You own, if any, only the magnetic media on which the Software has been delivered. It is an express condition of this Agreement that the title and ownership of the Software shall be retained by its owners.
Copying
The Software and its documentation are the subject of Copyright.
You may not make any copies nor cause others to make copies of the Software except such copies as are necessary for licensed use and one copy for operational security. Any such copies are subject to the conditions of this Agreement.
You may not modify, adapt, merge, translate, reverse engineer, decompile, disassemble or create derivative works based on the whole or any part of the Software or its associated documentation.
You may be held legally responsible for any copyright infringement, unauthorized transfer, reproduction or use of the Software or its documentation.
Limitation of Warranty
The media, if any, not the Software contained therein, is warranted to the original purchaser against defects in material and workmanship for a period of one year from the date of original purchase. Defective media will be replaced when it is returned to your supplier, postage prepaid, along with a copy of the purchase receipt.
THESE RIGHTS ARE YOUR SOLE AND EXCLUSIVE REMEDY, WHETHER IN TORT, CONTRACT, OR OTHERWISE. IN NO EVENT SHALL SUPPLIER, OWNER OF THE SOFTWARE OR ITS LICENSORS BE LIABLE FOR DAMAGES (INCLUDING ANY FOR LOSS OF INFORMATION, PROFITS, SAVINGS OR BUSINESS INTERRUPTION OR OTHER DIRECT, INDIRECT, INCIDENTAL, CONSEQUENTIAL OR SPECIAL DAMAGES) ARISING OUT OF THE SOFTWARE OR THE USE THEREOF, OR THE INABILITY TO USE THE SOFTWARE.
Exporting Law
You acknowledge that the export of the Software is governed by the export control laws of the United States and other countries. You agree to comply with all such export control laws.
Governing Law and Jurisdiction
If any provision or portion of this Agreement shall be found to be illegal, invalid or unenforceable, the remaining provisions shall remain in full force and effect. This Agreement shall be governed by the laws of California, USA and is subject to the jurisdiction of the Federal District courts for the Central District of California by a judge and not a jury.

#### INTRODUCTION

This file describes how to set up your printer driver and contains the most up-to-date information that was available at the time of software release. Please see [2] Limitation/Notes in using PCL5 printer driver section for details of known limitations. For information on printer driver settings and features, please check the Help file.
Please make sure to read this before installing PCL printer driver.

#### CONTENTS

[1] How to install PCL printer driver
(1) Installing PCL printer driver at the first time
(2) Upgrading the PCL printer driver
(3) Uninstalling the PCL printer driver
(4) Notes for the installation
(5) Notes for the upgrading
[2] Limitation/Notes in using PCL5 printer driver

#### [1] How to install PCL printer driver

(1) Installing PCL printer driver at the first time
Notes:
All applications must be closed before installing the driver.
This procedure requires administrator privileges (admin account or "Run as Administrator").
(1-1) Windows 10/Server 2016/Server 2019

1. From the Start menu, add a printer by navigating one of the following:
   a. "Settings" > "Devices" > "Printers & scanners" > "Add printers & scanners" or,
   b. "All Apps" (skip for Windows Server 2016/Server 2019 )> "Windows System" > "Control Panel" > "View devices and printers" > "Add a printer".
2. From "Add printers & scanners" or "Choose a device or printer to add to this PC", click "The printer that I want isn't listed".
3. Select the connection method in "Find a printer by other options" according to the printer setup wizard. The following is the procedure when "Add a local printer or network printer with manual settings" is selected.
   Below is the procedure when "Add a local printer or network printer with manual settings" is selected.
4. Select a printer port in the "Choose a printer port" dialog.
   a. If an existing port will be used, select it from the "Use an existing port:" dropdown list.
   b. If a new port will be used, choose "Standard TCP/IP Port" from the "Create a new port:" dropdown list. In the "Type a printer hostname or IP address" dialog, enter the hostname or IP address and uncheck "Query the printer and automatically select the driver to use".
5. Specify the .inf driver file under the disk1 directory of the downloaded driver folder or by installing the CD-ROM and then click "Have Disk".
6. Select the appropriate manufacturer and printer in the "Install the printer driver" dialog.
7. Enter a printer name in the "Type a printer name" dialog.
8. Select if the printer should be shared with other network users in the "Printer Sharing" dialog.
9. Check "Set as the default printer" in the "You've successfully added [Printer name]" dialog if the printer should be used as the default printer.
10. Check if the printer is working properly by clicking "Print a test page" in the "You've successfully added [Printer name]" dialog.
11. Click "Finish" to complete the driver installation.

(1-2) Windows 8.1/Server 2012/Server 2012 R2

1. Initialize the "Add Printer" dialog by navigating to the following from the Charms Bar: "Settings" > "Control Panel" > "View devices and printers" > "Add a printer".
2. Stop searching for available printers and select "The printer that I want isn't listed" in the "Select a printer" dialog.
3. Select the connection method in "Find a printer by other options" dialog.
   Below is the procedure when "Add a local printer or network printer with manual settings" is selected.
4. Select a printer port in the "Choose a printer port" dialog.
   a. If an existing port will be used, select it from the "Use an existing port:" dropdown list.
   b. If a new port will be used, select "Standard TCP/IP Port" from the "Create a new port:" dropdown lists. Enter the device IP address and uncheck "Query the printer and automatically select the driver to use" in the "Type a printer hostname or IP address" dialog.
5. Specify the .inf driver file under the disk1 directory of the downloaded driver folder or included in the CD-ROM-by clicking "Have Disk".
6. Select the appropriate manufacturer and printer in the "Install the printer driver" dialog.
7. Enter a printer name in the "Type a printer name" dialog.
8. Select if the printer should be shared with other network users in the "Printer Sharing" dialog.
9. Check "Set as the default printer" in the "You've successfully added [Printer name]" dialog if the printer should be used as the default.
10. You can check if the printer is working properly by clicking "Print a test page" in the "You've successfully added [Printer name]" dialog.
11. Click "Finish" to complete the driver installation.

(1-3) Windows Server 2008

1. Initialize the "Add Printer" dialog by navigating to the following from the Start button: "Printers" > "Add a Printer".
2. Select the connection method in the "What type of printer do you want to install?" dialog.
   Below is the procedure when "Add a local printer" is selected.
3. Select a printer port in the "Choose a printer port" dialog.
   a. If an existing port will be used, select it from the "Use an existing port:" dropdown list.
   b. If a new port will be used, select "Standard TCP/IP Port" from the "Create a new port:" dropdown list. Enter the device IP address and uncheck the "Query the printer and automatically select the driver to use" in the "Type a printer hostname or IP address" dialog.
4. Specify the .inf driver file under the disk1 directory of the downloaded driver folder or included in the CD-ROM-by clicking "Have Disk".
5. Select the appropriate manufacturer and printer in the "Install the printer driver" dialog.
6. Enter a printer name and check "Set as the default printer" if the printer should be used as the default in the "Type a printer name" dialog,
7. Select if the printer should be shared with other network users in the "Printer Sharing" dialog.
8. You can check if the printer is working properly by clicking "Print a test page" in the "You've successfully added [Printer name]" dialog.
9. Click "Finish" to complete the driver installation.

(1-4) Windows Windows 7/Server 2008 R2

1. Initialize the "Add Printer" dialog by navigating to the following from the Start button: "Devices and Printers" > "Add a Printer".
2. Select the connection method in the "What type of printer do you want to install?" dialog.
   Below is the procedure when "Add a local printer" is selected.
3. Select a printer port in the "Choose a printer port" dialog.
   a. If an existing port will be used, select it from the "Use an existing port:" dropdown list.
   b. If a new port will be used, select "Standard TCP/IP Port" from the "Create a new port:" dropdown list. Enter the device IP address and uncheck the "Query the printer and automatically select the driver to use" in the "Type a printer hostname or IP address" dialog.
4. Specify the .inf driver file under the disk1 directory of the downloaded driver folder or included in the CD-ROM-by clicking "Have Disk".
5. Select the appropriate manufacturer and printer in the "Install the printer driver" dialog.
6. Enter a printer name in the "Type a printer name" dialog.
7. Select if the printer should be shared with other network users in the "Printer Sharing" dialog.
8. Check "Set as the default printer" in the "You've successfully added [Printer name]" dialog if the printer should be used as the default.
9. You can check if the printer is working properly by clicking "Print a test page" in the "You've successfully added [Printer name]" dialog.
10. Click "Finish" to complete the driver installation.

(2) Upgrading the PCL printer driver
Notes:
All applications must be closed before upgrading the driver.
This procedure requires administrator privileges (admin account or "Run as Administrator").

1. Press the [Start] button; navigate to [Settings] or [Control Panel]; click [Printers], [Printers and Faxes], [View Devices and Printers], [Devices and Printers], or [Devices].
2. Open the Properties of the printer to be upgraded.
3. Click "New Driver" button on "Advanced" tab. Then click "Next".
4. Select "Have Disk..." then browse to the folder containing the extracted printer driver INF file. Click "Open".
5. Click "OK" and select the printer model. Click "Next".
6. Once the installation is complete, click "Finish".
7. Click "OK" to close the printer properties dialog box.

(3) Uninstalling the PCL printer driver
Notes:
All applications must be closed before uninstalling the driver.
This procedure requires administrator privileges (admin account or "Run as Administrator").
(3-1) Windows 7/8.1/10/Server 2008 R2/Server 2012/Server 2012 R2/Server 2016/Server 2019

1. Open the "Printers" folder (or "Devices and Printers").
2. Delete the printer icon corresponding to the driver that is to be uninstalled.
3. Print server properties > Driver tab.
4. Select the driver to be uninstalled.
5. Press the Remove key.
6. Press "Remove driver and driver package".
7. Restart the PC.

(3-2) Windows Server 2008

1. Open the "Printers" folder (or "Printers and Faxes").
2. Delete the printer icon corresponding to the driver that is to be uninstalled.
3. Right click in the "Printers" folder and select "Run as Administrator".
4. Server Properties > Driver tab.
5. Select the driver to be uninstalled.
6. Press the Remove key.
7. Press "Remove driver and driver package".
8. Restart the PC.

(4) Notes for the installation

* | With PCL printer driver, the drivers of different versions can't be used together.
* | If "Print Settings" screen doesn't look normal after installation, delete the driver with the procedure of above (3) and reinstall the driver.
* | Do not extract CD-ROM before the installation is finished. Or else, system error might occur.
* | During the driver installation, Windows may suggest to keep the newer module already installed in Windows. Please select "Yes" to use the newer module.
* | The CD-ROM installer causes the Spooler service to temporarily stop. We do not recommend using the CD-ROM installer on a member server of a Microsoft cluster environment because other services that rely on the Spooler might also stop causing a failover to occur. Instead, the Add Printer Wizard should be used. If this is done, the Spooler service will not stop.

(5) Notes for the upgrading

* | The settings of overwritten PCL5 drivers will not be inherited.
* | An upgrade can only be performed between drivers of the same model and type of PCL (PCL5e, PCL5c).

#### [2] Limitation/Notes in using PCL5 printer driver

The settings which are introduced below are depending on the printer or the printer driver you use.

[In General]

* To avoid problems in general, make sure that there is plenty of free disk space.
* With some applications (e.g. CorelDRAW, Visio), complicated images may take a long time to print.
* If the printer driver language differs from that of the Operating System, characters may not be printed properly or the characters on the printer driver may not be displayed properly.

[OS/Windows Related Issues]

* | When the spooler is paused, please do not send the print job.
* | If a Separator Page is selected, some documents may not print as expected.
* | Please do not change the "Driver" setting on the "General" or "Advanced Options" tab.

[With Driver Settings]

* [Copies] in [Setup] Tab:
When "Copies" is selected on the driver's "Setup" tab, the value may not be reflected in the application print dialog box. Be sure to set the number of copies only in the driver, not in the application.
* [Staple] in [Setup] Tab:
Documents may not be stapled at the slant angle, even when you select "Top Left Slant" or "Top Right Slant". In such a case, the document will be stapled parallel to an edge of the paper.
* [Custom Paper Size] in [Paper] Tab:
The measurement unit in the Custom Paper Size dialog is reset to "cm" when the driver dialog is reopened, even if the custom paper size was previously specified in "inch". The paper size specification is retained regardless of the unit.
A paper mismatch error might occur when the measurement unit in the Custom Paper Size dialog is different from the Custom Size setting on the printer operation panel.
* [On first page only] in [Watermark] Tab, and [Booklet/Duplex] in [Setup] Tab:
The watermark is not printed on the first page when both "On first page only" and "Booklet" are selected.
* [Print Quality] Tab:
I f the "TrueType Mode" is set to "Download as bit image", the watermark may not print correctly.
* [Booklet/Duplex] in [Setup] Tab:
Printing a large document in booklet, duplex or reverse order printing produce a large temporary file. If you encounter an error when printing a large document in booklet, try again after increasing the free area in system installed drive (e.g. C:).
* [Edge to Edge Print] in [Print Quality] Tab, and [Non Reduction Booklet] in [Setup] Tab:
When both "Edge to Edge Print" and "Non Reduction Booklet" functions are selected, some documents may not print as expected.
* [Covers] in [Paper] Tab:
Use of a different Paper Source for the cover setting might result in a paper mismatch error. This occurs if the cover is of a different paper size than the rest of the document. This only happens if the cover is not blank and if the source tray for the rest of the document is not "Auto Tray Select". As a workaround, change the print settings so that any one of the above conditions are not met. Note: "cover" = Front Cover, Back Cover or Chaptering Pages
* [Print Banner Page] in [Valid Access] Tab:
The first 15 bytes of the hostname can be printed on the banner page.
Banner pages cannot be printed using the source tray that is selected to print "Chapter Page". Please use another source tray to print banner pages.

[Graphics/Images]

* When graphics images or text printed as graphics images are not printed as they appear on your computer screen, change the "Graphics Mode" on the "Print Quality" tab.
* Selecting the Spool Type as EMF may cause some applications not to print well in "Vector" mode. If this happens, return the Spool Type setting to RAW.

[Fonts/Texts]

* With Adobe Type Manager(ATM), some characters may not print correctly. To avoid this problem, print the document with PCL 6 or PostScript driver.
* With some applications, some characters may not print correctly. To solve this problem, change the "TrueType Mode" and/or the "Use Printer Fonts" on the "Print Quality" tab.
* Documents that contain fonts not installed on your computer will not print correctly. Make sure your document only contains fonts installed on your computer.
* The watermark as "As Outline only" may not print if the watermark message contains Chinese characters. To avoid this problem, use the PCL 6 driver.
* Additional lines may appear when the bold HANYI fonts larger than 36 points are printed.
* The HANYI fonts can not be printed in 300 dpi. To avoid this problem, print it in 600 dpi.
* To print watermark text in Chinese, choose a Chinese font.
* If the language of the filename of the data that is to be printed does not match the language of the driver UI, the filename might not be displayed correctly on the operation panel.

[Connection/Port related Issues]

* | When printing complicated documents to a printer connected with a parallel interface, the printer time-out may cause the document to print incorrectly. If this happens, set the Spool Setting to "Start printing after last page is spooled" and/or extend the IO timeout at the printer operation panel(max. 300 seconds).
* | When the printer is connected with a SMB port, "Update Now" in the Accessories tab doesn't work. Please manually configure the accessories.

[CMYK used for Black and White Documents]

* | Black and White documents might be printed in full color (CMYK). To ensure that the job prints using pure Black (K), please change the color mode to "Black and White".
* | When selecting "Color" from "Color/ Black and White" setting in the "Setup" Tab, black and white document may be printed as a color job, depending on application or data. If you want to print a document in black and white, select "Black and White" in "Color/ Black and White" setting.

[Help issues]

* | When resolution setting of Display is smaller than 800x600dpi, "Information Help" window dialog may be oversized on the display. In this case, to close the window, click "X" button on the right corner of the window dialog.

[Other issues]

* | Additional Page Count in Duplex Printing An extra page is added to the end of odd-paged duplex jobs. The added page might be incremented in the printer's counter.
* | Point&Print drivers do not inherit Watermark settings Drivers installed on a client using Point&Print do not inherit Watermark settings from the server.
* | Reverse Order is not supported with the Duplex, Front Cover, Back Cover, Chapter Pages, Slip Sheet functions.

[Application issues]

* | Microsoft * Microsoft Office XP * - If you are using Office XP, be sure to apply Service Pack 1 or later to avoid printing problems. * MS-Project * - When using with MS-Project, the stripe pattern interval may not print as it appears on your computer screen. If this happens, change the "Graphics Mode". - To print multiple copies from MS-Project, set the number of copies setting in the application print dialog box to 1, and then specify the number of copies using "Copies" setting on the driver's "Setup" tab. - Some applications merge multiple copies of a document into a single copy. This results in the following: - Output copies are not correctly shifted or rotated. - All of the copies are stapled, folded, or bound together if the staple, fold, or perfect binding function is used. Examples of such applications include Microsoft Project and Microsoft Visio. * PowerPoint * - PowerPoint may print some graphics objects with the same color although they are in different colors on the computer screen. To solve this problem, change the object's color. * WordPad - When you change the printer properties from WordPad, changes will not be reflected in the print job immediately following the change.
* | Corel * CorelDRAW * - You can not enter the number of copies greater than 9 in the printer driver dialog opened from CorelDRAW 8, due to a problem in CorelDRAW 8. To print more than 9 copies, set the number of copies in the CorelDRAW 8's print dialog. - The printer driver dialog opened from CorelDRAW 8 may show unreadable characters, due to a problem in CorelDRAW 8.
* | Adobe * Acrobat * - If printed using Adobe Acrobat/Acrobat Reader, black and white PDF documents compressed by MMR are printed in full color with some image distortion/deterioration. This can be prevented by disabling the application's "Print As Image" function. - Adobe Reader might add an extra page of padding to the end of odd-paged duplex documents. This will be counted as a BW page. When application's copies is 1 and PCL5 driver's copies is 2 or more, the extra page is not added. - The number of copies specified in the driver UI might not be reflected in the application print dialog when printing from any of the following applications: - Adobe Reader - Adobe Acrobat - Adobe Illustrator - Adobe InDesign Because of this, the output number of copies is different from the expected result. Workaround: Set the number of copies in the application print dialog. * Frame Maker * - With Adobe Frame Maker, please use *.FM document to print when "Duplex/Booklet" or "Staple" function is selected. * Page Maker * - PageMaker may not print graphics if a document contains large amount of graphics. To print such documents, change the "Memory Usage" settings to "Font Priority" on the printer operation panel. - PageMaker shifts the image by about one inch with some paper sizes. To solve this problem, print using a different paper size.

All brand names and product names mentioned in this document are trademarks or registered trademarks of their respective companies.